<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.2.0">
<drawing>
<board>
<plain>
<wire x1="300" y1="0" x2="300" y2="200" width="0" layer="20"/>
<wire x1="300" y1="200" x2="0" y2="200" width="0" layer="20"/>
<hole x="4.91" y="195.08" drill="3.2"/>
<hole x="149.94" y="194.98" drill="3.2"/>
<hole x="294.91" y="195.01" drill="3.2"/>
<hole x="295.01" y="5.01" drill="3.2"/>
<hole x="4.98" y="5.01" drill="3.2"/>
<hole x="29.88" y="100.12" drill="5.5"/>
<hole x="295.01" y="99.99" drill="3.2"/>
<hole x="120.03" y="69.46" drill="3.2"/>
<hole x="180.03" y="69.46" drill="3.2"/>
<hole x="120.03" y="10.46" drill="3.2"/>
<hole x="180.03" y="10.46" drill="3.2"/>
<wire x1="0" y1="0" x2="0" y2="200" width="0" layer="20"/>
<hole x="269.88" y="100.12" drill="5.5"/>
<hole x="89.88" y="170.12" drill="5.5"/>
<hole x="209.88" y="170.12" drill="5.5"/>
<hole x="89.88" y="30.12" drill="5.5"/>
<hole x="209.88" y="30.12" drill="5.5"/>
<hole x="194.88" y="100.12" drill="5.5"/>
<hole x="104.88" y="100.12" drill="5.5"/>
<wire x1="0" y1="0" x2="300" y2="0" width="0" layer="20"/>
<text>DC jack</text>
<text>Power Switch</text>
<text>Fuse 3.5 Amps</text>
<text>V_in:
4 .. 25 V DC</text>
<text>PLAYER A</text>
<text>PLAYER B</text>
<text>PLAYER D</text>
<text>PLAYER C</text>
<text>PDI</text>
<text>SPI</text>
<text>SPI</text>
<text>SPI</text>
<text>SPI</text>
<text>USB</text>
<text>SPI (ISP)</text>
<text>GND</text>
<text>!RES</text>
<text>VCC</text>
<text>SCK</text>
<text>PDI</text>
<text>GND</text>
<text>CLK</text>
<text>VCC</text>
<text>DATA</text>
<text>MOSI</text>
<text>MISO</text>
<text>1</text>
<text>1</text>
<text>USB</text>
<text>GND</text>
<text>VCC</text>
<text>D-</text>
<text>D+</text>
<text>DART SCORER</text>
<text>2015 Julian Krämer</text>
<text>github.com/tuxoid/dartscorer</text>
</plain>
<libraries>
<library name="resistor">
<description>&lt;b&gt;Resistors, Capacitors, Inductors&lt;/b&gt;&lt;p&gt;
Based on the previous libraries:
&lt;ul&gt;
&lt;li&gt;r.lbr
&lt;li&gt;cap.lbr 
&lt;li&gt;cap-fe.lbr
&lt;li&gt;captant.lbr
&lt;li&gt;polcap.lbr
&lt;li&gt;ipc-smd.lbr
&lt;/ul&gt;
All SMD packages are defined according to the IPC specifications and  CECC&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;p&gt;
&lt;p&gt;
for Electrolyt Capacitors see also :&lt;p&gt;
www.bccomponents.com &lt;p&gt;
www.panasonic.com&lt;p&gt;
www.kemet.com&lt;p&gt;
&lt;p&gt;
for trimmer refence see : &lt;u&gt;www.electrospec-inc.com/cross_references/trimpotcrossref.asp&lt;/u&gt;&lt;p&gt;

&lt;map name="nav_main"&gt;
&lt;area shape="rect" coords="0,1,140,23" href="../military_specs.asp" title=""&gt;
&lt;area shape="rect" coords="0,24,140,51" href="../about.asp" title=""&gt;
&lt;area shape="rect" coords="1,52,140,77" href="../rfq.asp" title=""&gt;
&lt;area shape="rect" coords="0,78,139,103" href="../products.asp" title=""&gt;
&lt;area shape="rect" coords="1,102,138,128" href="../excess_inventory.asp" title=""&gt;
&lt;area shape="rect" coords="1,129,138,150" href="../edge.asp" title=""&gt;
&lt;area shape="rect" coords="1,151,139,178" href="../industry_links.asp" title=""&gt;
&lt;area shape="rect" coords="0,179,139,201" href="../comments.asp" title=""&gt;
&lt;area shape="rect" coords="1,203,138,231" href="../directory.asp" title=""&gt;
&lt;area shape="default" nohref&gt;
&lt;/map&gt;

&lt;html&gt;

&lt;title&gt;&lt;/title&gt;

 &lt;LINK REL="StyleSheet" TYPE="text/css" HREF="style-sheet.css"&gt;

&lt;body bgcolor="#ffffff" text="#000000" marginwidth="0" marginheight="0" topmargin="0" leftmargin="0"&gt;
&lt;table border=0 cellspacing=0 cellpadding=0 width="100%" cellpaddding=0 height="55%"&gt;
&lt;tr valign="top"&gt;

&lt;/td&gt;
&lt;! &lt;td width="10"&gt;&amp;nbsp;&lt;/td&gt;
&lt;td width="90%"&gt;

&lt;b&gt;&lt;font color="#0000FF" size="4"&gt;TRIM-POT CROSS REFERENCE&lt;/font&gt;&lt;/b&gt;
&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=2&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;RECTANGULAR MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BOURNS&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;BI&amp;nbsp;TECH&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;DALE-VISHAY&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PHILIPS/MEPCO&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MURATA&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;PANASONIC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;SPECTROL&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;B&gt;
      &lt;FONT SIZE=3 FACE=ARIAL color="#FF0000"&gt;MILSPEC&lt;/FONT&gt;
      &lt;/B&gt;
    &lt;/TD&gt;&lt;TD&gt;&amp;nbsp;&lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3 &gt;
      3005P&lt;BR&gt;
      3006P&lt;BR&gt;
      3006W&lt;BR&gt;
      3006Y&lt;BR&gt;
      3009P&lt;BR&gt;
      3009W&lt;BR&gt;
      3009Y&lt;BR&gt;
      3057J&lt;BR&gt;
      3057L&lt;BR&gt;
      3057P&lt;BR&gt;
      3057Y&lt;BR&gt;
      3059J&lt;BR&gt;
      3059L&lt;BR&gt;
      3059P&lt;BR&gt;
      3059Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      89P&lt;BR&gt;
      89W&lt;BR&gt;
      89X&lt;BR&gt;
      89PH&lt;BR&gt;
      76P&lt;BR&gt;
      89XH&lt;BR&gt;
      78SLT&lt;BR&gt;
      78L&amp;nbsp;ALT&lt;BR&gt;
      56P&amp;nbsp;ALT&lt;BR&gt;
      78P&amp;nbsp;ALT&lt;BR&gt;
      T8S&lt;BR&gt;
      78L&lt;BR&gt;
      56P&lt;BR&gt;
      78P&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      T18/784&lt;BR&gt;
      783&lt;BR&gt;
      781&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2199&lt;BR&gt;
      1697/1897&lt;BR&gt;
      1680/1880&lt;BR&gt;
      2187&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      8035EKP/CT20/RJ-20P&lt;BR&gt;
      -&lt;BR&gt;
      RJ-20X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      1211L&lt;BR&gt;
      8012EKQ&amp;nbsp;ALT&lt;BR&gt;
      8012EKR&amp;nbsp;ALT&lt;BR&gt;
      1211P&lt;BR&gt;
      8012EKJ&lt;BR&gt;
      8012EKL&lt;BR&gt;
      8012EKQ&lt;BR&gt;
      8012EKR&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      2101P&lt;BR&gt;
      2101W&lt;BR&gt;
      2101Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      2102L&lt;BR&gt;
      2102S&lt;BR&gt;
      2102Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVMCOG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      43P&lt;BR&gt;
      43W&lt;BR&gt;
      43Y&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      40L&lt;BR&gt;
      40P&lt;BR&gt;
      40Y&lt;BR&gt;
      70Y-T602&lt;BR&gt;
      70L&lt;BR&gt;
      70P&lt;BR&gt;
      70Y&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      RT/RTR12&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;
      RJ/RJR12&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SQUARE MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
   &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3250L&lt;BR&gt;
      3250P&lt;BR&gt;
      3250W&lt;BR&gt;
      3250X&lt;BR&gt;
      3252P&lt;BR&gt;
      3252W&lt;BR&gt;
      3252X&lt;BR&gt;
      3260P&lt;BR&gt;
      3260W&lt;BR&gt;
      3260X&lt;BR&gt;
      3262P&lt;BR&gt;
      3262W&lt;BR&gt;
      3262X&lt;BR&gt;
      3266P&lt;BR&gt;
      3266W&lt;BR&gt;
      3266X&lt;BR&gt;
      3290H&lt;BR&gt;
      3290P&lt;BR&gt;
      3290W&lt;BR&gt;
      3292P&lt;BR&gt;
      3292W&lt;BR&gt;
      3292X&lt;BR&gt;
      3296P&lt;BR&gt;
      3296W&lt;BR&gt;
      3296X&lt;BR&gt;
      3296Y&lt;BR&gt;
      3296Z&lt;BR&gt;
      3299P&lt;BR&gt;
      3299W&lt;BR&gt;
      3299X&lt;BR&gt;
      3299Y&lt;BR&gt;
      3299Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      -&lt;BR&gt;
      64P&amp;nbsp;ALT&lt;BR&gt;
      64W&amp;nbsp;ALT&lt;BR&gt;
      64X&amp;nbsp;ALT&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      66X&amp;nbsp;ALT&lt;BR&gt;
      66P&amp;nbsp;ALT&lt;BR&gt;
      66W&amp;nbsp;ALT&lt;BR&gt;
      66P&lt;BR&gt;
      66W&lt;BR&gt;
      66X&lt;BR&gt;
      67P&lt;BR&gt;
      67W&lt;BR&gt;
      67X&lt;BR&gt;
      67Y&lt;BR&gt;
      67Z&lt;BR&gt;
      68P&lt;BR&gt;
      68W&lt;BR&gt;
      68X&lt;BR&gt;
      67Y&amp;nbsp;ALT&lt;BR&gt;
      67Z&amp;nbsp;ALT&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      5050&lt;BR&gt;
      5091&lt;BR&gt;
      5080&lt;BR&gt;
      5087&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T63YB&lt;BR&gt;
      T63XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      5887&lt;BR&gt;
      5891&lt;BR&gt;
      5880&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T93Z&lt;BR&gt;
      T93YA&lt;BR&gt;
      T93XA&lt;BR&gt;
      T93YB&lt;BR&gt;
      T93XB&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKW&lt;BR&gt;
      8026EKM&lt;BR&gt;
      8026EKP&lt;BR&gt;
      8026EKB&lt;BR&gt;
      8026EKM&lt;BR&gt;
      1309X&lt;BR&gt;
      1309P&lt;BR&gt;
      1309W&lt;BR&gt;
      8024EKP&lt;BR&gt;
      8024EKW&lt;BR&gt;
      8024EKN&lt;BR&gt;
      RJ-9P/CT9P&lt;BR&gt;
      RJ-9W&lt;BR&gt;
      RJ-9X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      3103P&lt;BR&gt;
      3103Y&lt;BR&gt;
      3103Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3105P/3106P&lt;BR&gt;
      3105W/3106W&lt;BR&gt;
      3105X/3106X&lt;BR&gt;
      3105Y/3106Y&lt;BR&gt;
      3105Z/3105Z&lt;BR&gt;
      3102P&lt;BR&gt;
      3102W&lt;BR&gt;
      3102X&lt;BR&gt;
      3102Y&lt;BR&gt;
      3102Z&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMCBG&lt;BR&gt;
      EVMCCG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      55-1-X&lt;BR&gt;
      55-4-X&lt;BR&gt;
      55-3-X&lt;BR&gt;
      55-2-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      50-2-X&lt;BR&gt;
      50-4-X&lt;BR&gt;
      50-3-X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      64P&lt;BR&gt;
      64W&lt;BR&gt;
      64X&lt;BR&gt;
      64Y&lt;BR&gt;
      64Z&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RT/RTR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RJ/RJR22&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RT/RTR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RJ/RJR26&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RT/RTR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      RJ/RJR24&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=8&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MURATA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;SPECTROL&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD ALIGN=CENTER&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;MILSPEC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3323P&lt;BR&gt;
      3323S&lt;BR&gt;
      3323W&lt;BR&gt;
      3329H&lt;BR&gt;
      3329P&lt;BR&gt;
      3329W&lt;BR&gt;
      3339H&lt;BR&gt;
      3339P&lt;BR&gt;
      3339W&lt;BR&gt;
      3352E&lt;BR&gt;
      3352H&lt;BR&gt;
      3352K&lt;BR&gt;
      3352P&lt;BR&gt;
      3352T&lt;BR&gt;
      3352V&lt;BR&gt;
      3352W&lt;BR&gt;
      3362H&lt;BR&gt;
      3362M&lt;BR&gt;
      3362P&lt;BR&gt;
      3362R&lt;BR&gt;
      3362S&lt;BR&gt;
      3362U&lt;BR&gt;
      3362W&lt;BR&gt;
      3362X&lt;BR&gt;
      3386B&lt;BR&gt;
      3386C&lt;BR&gt;
      3386F&lt;BR&gt;
      3386H&lt;BR&gt;
      3386K&lt;BR&gt;
      3386M&lt;BR&gt;
      3386P&lt;BR&gt;
      3386S&lt;BR&gt;
      3386W&lt;BR&gt;
      3386X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      25P&lt;BR&gt;
      25S&lt;BR&gt;
      25RX&lt;BR&gt;
      82P&lt;BR&gt;
      82M&lt;BR&gt;
      82PA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      91E&lt;BR&gt;
      91X&lt;BR&gt;
      91T&lt;BR&gt;
      91B&lt;BR&gt;
      91A&lt;BR&gt;
      91V&lt;BR&gt;
      91W&lt;BR&gt;
      25W&lt;BR&gt;
      25V&lt;BR&gt;
      25P&lt;BR&gt;
      -&lt;BR&gt;
      25S&lt;BR&gt;
      25U&lt;BR&gt;
      25RX&lt;BR&gt;
      25X&lt;BR&gt;
      72XW&lt;BR&gt;
      72XL&lt;BR&gt;
      72PM&lt;BR&gt;
      72RX&lt;BR&gt;
      -&lt;BR&gt;
      72PX&lt;BR&gt;
      72P&lt;BR&gt;
      72RXW&lt;BR&gt;
      72RXL&lt;BR&gt;
      72X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      T7YB&lt;BR&gt;
      T7YA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      TXD&lt;BR&gt;
      TYA&lt;BR&gt;
      TYP&lt;BR&gt;
      -&lt;BR&gt;
      TYD&lt;BR&gt;
      TX&lt;BR&gt;
      -&lt;BR&gt;
      150SX&lt;BR&gt;
      100SX&lt;BR&gt;
      102T&lt;BR&gt;
      101S&lt;BR&gt;
      190T&lt;BR&gt;
      150TX&lt;BR&gt;
      101&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      101SX&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ET6P&lt;BR&gt;
      ET6S&lt;BR&gt;
      ET6X&lt;BR&gt;
      RJ-6W/8014EMW&lt;BR&gt;
      RJ-6P/8014EMP&lt;BR&gt;
      RJ-6X/8014EMX&lt;BR&gt;
      TM7W&lt;BR&gt;
      TM7P&lt;BR&gt;
      TM7X&lt;BR&gt;
      -&lt;BR&gt;
      8017SMS&lt;BR&gt;
      -&lt;BR&gt;
      8017SMB&lt;BR&gt;
      8017SMA&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      CT-6W&lt;BR&gt;
      CT-6H&lt;BR&gt;
      CT-6P&lt;BR&gt;
      CT-6R&lt;BR&gt;
      -&lt;BR&gt;
      CT-6V&lt;BR&gt;
      CT-6X&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKV&lt;BR&gt;
      -&lt;BR&gt;
      8038EKX&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      8038EKP&lt;BR&gt;
      8038EKZ&lt;BR&gt;
      8038EKW&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3321H&lt;BR&gt;
      3321P&lt;BR&gt;
      3321N&lt;BR&gt;
      1102H&lt;BR&gt;
      1102P&lt;BR&gt;
      1102T&lt;BR&gt;
      RVA0911V304A&lt;BR&gt;
      -&lt;BR&gt;
      RVA0911H413A&lt;BR&gt;
      RVG0707V100A&lt;BR&gt;
      RVA0607V(H)306A&lt;BR&gt;
      RVA1214H213A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      3104B&lt;BR&gt;
      3104C&lt;BR&gt;
      3104F&lt;BR&gt;
      3104H&lt;BR&gt;
      -&lt;BR&gt;
      3104M&lt;BR&gt;
      3104P&lt;BR&gt;
      3104S&lt;BR&gt;
      3104W&lt;BR&gt;
      3104X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      EVMQ0G&lt;BR&gt;
      EVMQIG&lt;BR&gt;
      EVMQ3G&lt;BR&gt;
      EVMS0G&lt;BR&gt;
      EVMQ0G&lt;BR&gt;
      EVMG0G&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMK4GA00B&lt;BR&gt;
      EVM30GA00B&lt;BR&gt;
      EVMK0GA00B&lt;BR&gt;
      EVM38GA00B&lt;BR&gt;
      EVMB6&lt;BR&gt;
      EVLQ0&lt;BR&gt;
      -&lt;BR&gt;
      EVMMSG&lt;BR&gt;
      EVMMBG&lt;BR&gt;
      EVMMAG&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMMCS&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM0&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      EVMM3&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      62-3-1&lt;BR&gt;
      62-1-2&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67R&lt;BR&gt;
      -&lt;BR&gt;
      67P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      67X&lt;BR&gt;
      63V&lt;BR&gt;
      63S&lt;BR&gt;
      63M&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63H&lt;BR&gt;
      63P&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      63X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      RJ/RJR50&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;&amp;nbsp;&lt;P&gt;
&lt;TABLE BORDER=0 CELLSPACING=1 CELLPADDING=3&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT color="#0000FF" SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SMD TRIM-POT CROSS REFERENCE&lt;/B&gt;&lt;/FONT&gt;
      &lt;P&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;MULTI-TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3224G&lt;BR&gt;
      3224J&lt;BR&gt;
      3224W&lt;BR&gt;
      3269P&lt;BR&gt;
      3269W&lt;BR&gt;
      3269X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      44G&lt;BR&gt;
      44J&lt;BR&gt;
      44W&lt;BR&gt;
      84P&lt;BR&gt;
      84W&lt;BR&gt;
      84X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST63Z&lt;BR&gt;
      ST63Y&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST5P&lt;BR&gt;
      ST5W&lt;BR&gt;
      ST5X&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;
      &lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;SINGLE TURN&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BOURNS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;BI&amp;nbsp;TECH&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;DALE-VISHAY&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PHILIPS/MEPCO&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;PANASONIC&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;TOCOS&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD&gt;
      &lt;FONT SIZE=3 FACE=ARIAL&gt;&lt;B&gt;AUX/KYOCERA&lt;/B&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
  &lt;TR&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      3314G&lt;BR&gt;
      3314J&lt;BR&gt;
      3364A/B&lt;BR&gt;
      3364C/D&lt;BR&gt;
      3364W/X&lt;BR&gt;
      3313G&lt;BR&gt;
      3313J&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      23B&lt;BR&gt;
      23A&lt;BR&gt;
      21X&lt;BR&gt;
      21W&lt;BR&gt;
      -&lt;BR&gt;
      22B&lt;BR&gt;
      22A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST5YL/ST53YL&lt;BR&gt;
      ST5YJ/5T53YJ&lt;BR&gt;
      ST-23A&lt;BR&gt;
      ST-22B&lt;BR&gt;
      ST-22&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      ST-4B&lt;BR&gt;
      ST-4A&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      ST-3B&lt;BR&gt;
      ST-3A&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      EVM-6YS&lt;BR&gt;
      EVM-1E&lt;BR&gt;
      EVM-1G&lt;BR&gt;
      EVM-1D&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      G4B&lt;BR&gt;
      G4A&lt;BR&gt;
      TR04-3S1&lt;BR&gt;
      TRG04-2S1&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;
      DVR-43A&lt;BR&gt;
      CVR-42C&lt;BR&gt;
      CVR-42A/C&lt;BR&gt;
      -&lt;BR&gt;
      -&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;
&lt;/TABLE&gt;
&lt;P&gt;
&lt;FONT SIZE=4 FACE=ARIAL&gt;&lt;B&gt;ALT =&amp;nbsp;ALTERNATE&lt;/B&gt;&lt;/FONT&gt;
&lt;P&gt;

&amp;nbsp;
&lt;P&gt;
&lt;/td&gt;
&lt;/tr&gt;
&lt;/table&gt;
&lt;/BODY&gt;&lt;/HTML&gt;</description>
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="SMC_D">
<description>&lt;b&gt;Chip Capacitor &lt;/b&gt; Polar tantalum capacitors with solid electrolyte&lt;p&gt;
Siemens Matsushita Components B 45 194, B 45 197, B 45 198&lt;br&gt;
Source: www.farnell.com/datasheets/247.pdf</description>
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
<package name="TQFP44">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt;</description>
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HC49/S">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="transistor">
<description>&lt;b&gt;Transistors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="0jlib">
<packages>
<package name="3DIGIT-7SEG">
</package>
<package name="KEYPAD">
</package>
<package name="EADOGL128S">
</package>
<package name="LED_RGB_PLCC6">
</package>
</packages>
</library>
<library name="fuse">
<description>&lt;b&gt;Fuses and Fuse Holders&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SH22,5">
<description>&lt;b&gt;FUSE HOLDER&lt;/b&gt;&lt;p&gt; grid 22,5 mm, OGN0031 8201 Schurter (Buerklin)</description>
</package>
</packages>
</library>
<library name="buzzer">
<description>&lt;b&gt;Speakers and Buzzers&lt;/b&gt;&lt;p&gt;
&lt;ul&gt;Distributors:
&lt;li&gt;Buerklin
&lt;li&gt;Spoerle
&lt;li&gt;Schukat
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="F/CM12P">
<description>&lt;b&gt;BUZZER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="st-microelectronics">
<description>&lt;b&gt;ST Microelectronics Devices&lt;/b&gt;&lt;p&gt;
Microcontrollers,  I2C components, linear devices&lt;p&gt;
http://www.st.com&lt;p&gt;
&lt;i&gt;Include st-microelectronics-2.lbr, st-microelectronics-3.lbr.&lt;p&gt;&lt;/i&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="HSOP8">
<description>&lt;b&gt;HSOP 08&lt;/b&gt; (Exposed pad)&lt;p&gt;
Source: http://www.st.com/internet/com/TECHNICAL_RESOURCES/TECHNICAL_LITERATURE/DATASHEET/CD00002851.pdf</description>
</package>
</packages>
</library>
<library name="con-cypressindustries">
<description>&lt;b&gt;Connectors from Cypress Industries&lt;/b&gt;&lt;p&gt;
www.cypressindustries.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="32005-201">
<description>&lt;b&gt;MINI USB-B R/A SMT W/ REAR&lt;/b&gt;&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/32005-201.pdf</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SMB">
<description>&lt;B&gt;DIODE&lt;/B&gt;</description>
</package>
<package name="SMBG">
<description>&lt;b&gt;DO-214AA GULL-WING&lt;/b&gt;&lt;p&gt;
Source: www.rsonline.de .. SMBJ12/C/15/C/24/C/30/C/5.0/C/7.5/C Voltage Suppressor. Data Sheet</description>
</package>
</packages>
</library>
<library name="inductor-coilcraft">
<description>&lt;b&gt;Coilcraft SMD Inductors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="DO3316P">
<description>&lt;b&gt;COILCRAFT&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1-1" library="resistor" package="C0805" value="100n"/>
<element name="C1-2" library="resistor" package="C0805" value="22p"/>
<element name="C1-3" library="resistor" package="C0805" value="22p"/>
<element name="IC1-1" library="avr-7" package="TQFP32-08" value="MEGA48/88/168-AU"/>
<element name="JP1-1" library="pinhead" package="2X03" value=""/>
<element name="LED1-1" library="led" package="CHIPLED_0805" value=""/>
<element name="LED1-2" library="led" package="CHIPLED_0805" value=""/>
<element name="LED1-3" library="led" package="CHIPLED_0805" value=""/>
<element name="LED1-4" library="led" package="CHIPLED_0805" value=""/>
<element name="Q1-1" library="crystal" package="HC49/S" value="20M">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="R0-1" library="resistor" package="R0805" value="10k"/>
<element name="R1-1" library="resistor" package="R0805" value="10k"/>
<element name="R1-10" library="resistor" package="R0805" value="5.6"/>
<element name="R1-11" library="resistor" package="R0805" value="5.6"/>
<element name="R1-12" library="resistor" package="R0805" value="5.6"/>
<element name="R1-13" library="resistor" package="R0805" value="5.6"/>
<element name="R1-14" library="resistor" package="R0805" value="5.6"/>
<element name="R1-15" library="resistor" package="R0805" value="5.6"/>
<element name="R1-16" library="resistor" package="R0805" value="5.6"/>
<element name="R1-17" library="resistor" package="R0805" value="5.6"/>
<element name="R1-2" library="resistor" package="R0805" value="10k"/>
<element name="R1-3" library="resistor" package="R0805" value="10k"/>
<element name="R1-4" library="resistor" package="R0805" value="750"/>
<element name="R1-5" library="resistor" package="R0805" value="100k"/>
<element name="R1-6" library="resistor" package="R0805" value="4.7"/>
<element name="R1-7" library="resistor" package="R0805" value="4.7"/>
<element name="R1-8" library="resistor" package="R0805" value="4.7"/>
<element name="R1-9" library="resistor" package="R0805" value="4.7"/>
<element name="T1-1" library="transistor" package="SOT23" value="BC846"/>
<element name="7SEG1" library="0jlib" package="3DIGIT-7SEG" value="3DIGIT-7SEG"/>
<element name="IC2-1" library="avr-7" package="TQFP32-08" value="MEGA48/88/168-AU"/>
<element name="R2-1" library="resistor" package="R0805" value="10k"/>
<element name="C2-3" library="resistor" package="C0805" value="22p"/>
<element name="C2-2" library="resistor" package="C0805" value="22p"/>
<element name="Q2-1" library="crystal" package="HC49/S" value="20M">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="C2-1" library="resistor" package="C0805" value="100n"/>
<element name="JP2-1" library="pinhead" package="2X03" value=""/>
<element name="R2-3" library="resistor" package="R0805" value="10k"/>
<element name="R2-2" library="resistor" package="R0805" value="10k"/>
<element name="T2-1" library="transistor" package="SOT23" value="BC846"/>
<element name="R2-4" library="resistor" package="R0805" value="750"/>
<element name="R2-5" library="resistor" package="R0805" value="100k"/>
<element name="R2-6" library="resistor" package="R0805" value="4.7"/>
<element name="R2-7" library="resistor" package="R0805" value="4.7"/>
<element name="R2-8" library="resistor" package="R0805" value="4.7"/>
<element name="R2-9" library="resistor" package="R0805" value="4.7"/>
<element name="LED2-1" library="led" package="CHIPLED_0805" value=""/>
<element name="LED2-2" library="led" package="CHIPLED_0805" value=""/>
<element name="LED2-3" library="led" package="CHIPLED_0805" value=""/>
<element name="LED2-4" library="led" package="CHIPLED_0805" value=""/>
<element name="7SEG2" library="0jlib" package="3DIGIT-7SEG" value="3DIGIT-7SEG"/>
<element name="R2-10" library="resistor" package="R0805" value="5.6"/>
<element name="R2-11" library="resistor" package="R0805" value="5.6"/>
<element name="R2-12" library="resistor" package="R0805" value="5.6"/>
<element name="R2-13" library="resistor" package="R0805" value="5.6"/>
<element name="R2-14" library="resistor" package="R0805" value="5.6"/>
<element name="R2-15" library="resistor" package="R0805" value="5.6"/>
<element name="R2-16" library="resistor" package="R0805" value="5.6"/>
<element name="R2-17" library="resistor" package="R0805" value="5.6"/>
<element name="KEYPAD" library="0jlib" package="KEYPAD" value="KEYPAD"/>
<element name="IC3-1" library="avr-7" package="TQFP32-08" value="MEGA48/88/168-AU"/>
<element name="R3-1" library="resistor" package="R0805" value="10k"/>
<element name="C3-3" library="resistor" package="C0805" value="22p"/>
<element name="C3-2" library="resistor" package="C0805" value="22p"/>
<element name="Q3-1" library="crystal" package="HC49/S" value="20M">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="C3-1" library="resistor" package="C0805" value="100n"/>
<element name="JP3-1" library="pinhead" package="2X03" value=""/>
<element name="R3-3" library="resistor" package="R0805" value="10k"/>
<element name="R3-2" library="resistor" package="R0805" value="10k"/>
<element name="T3-1" library="transistor" package="SOT23" value="BC846"/>
<element name="R3-4" library="resistor" package="R0805" value="750"/>
<element name="R3-5" library="resistor" package="R0805" value="100k"/>
<element name="R3-6" library="resistor" package="R0805" value="4.7"/>
<element name="R3-7" library="resistor" package="R0805" value="4.7"/>
<element name="R3-8" library="resistor" package="R0805" value="4.7"/>
<element name="R3-9" library="resistor" package="R0805" value="4.7"/>
<element name="LED3-1" library="led" package="CHIPLED_0805" value=""/>
<element name="LED3-2" library="led" package="CHIPLED_0805" value=""/>
<element name="LED3-3" library="led" package="CHIPLED_0805" value=""/>
<element name="LED3-4" library="led" package="CHIPLED_0805" value=""/>
<element name="7SEG3" library="0jlib" package="3DIGIT-7SEG" value="3DIGIT-7SEG"/>
<element name="R3-10" library="resistor" package="R0805" value="5.6"/>
<element name="R3-11" library="resistor" package="R0805" value="5.6"/>
<element name="R3-12" library="resistor" package="R0805" value="5.6"/>
<element name="R3-13" library="resistor" package="R0805" value="5.6"/>
<element name="R3-14" library="resistor" package="R0805" value="5.6"/>
<element name="R3-15" library="resistor" package="R0805" value="5.6"/>
<element name="R3-16" library="resistor" package="R0805" value="5.6"/>
<element name="R3-17" library="resistor" package="R0805" value="5.6"/>
<element name="IC4-1" library="avr-7" package="TQFP32-08" value="MEGA48/88/168-AU"/>
<element name="R4-1" library="resistor" package="R0805" value="10k"/>
<element name="C4-3" library="resistor" package="C0805" value="22p"/>
<element name="C4-2" library="resistor" package="C0805" value="22p"/>
<element name="Q4-1" library="crystal" package="HC49/S" value="20M">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="1667008"/>
</element>
<element name="C4-1" library="resistor" package="C0805" value="100n"/>
<element name="JP4-1" library="pinhead" package="2X03" value=""/>
<element name="R4-3" library="resistor" package="R0805" value="10k"/>
<element name="R4-2" library="resistor" package="R0805" value="10k"/>
<element name="T4-1" library="transistor" package="SOT23" value="BC846"/>
<element name="R4-4" library="resistor" package="R0805" value="750"/>
<element name="R4-5" library="resistor" package="R0805" value="100k"/>
<element name="R4-6" library="resistor" package="R0805" value="4.7"/>
<element name="R4-7" library="resistor" package="R0805" value="4.7"/>
<element name="R4-8" library="resistor" package="R0805" value="4.7"/>
<element name="R4-9" library="resistor" package="R0805" value="4.7"/>
<element name="LED4-1" library="led" package="CHIPLED_0805" value=""/>
<element name="LED4-2" library="led" package="CHIPLED_0805" value=""/>
<element name="LED4-3" library="led" package="CHIPLED_0805" value=""/>
<element name="LED4-4" library="led" package="CHIPLED_0805" value=""/>
<element name="7SEG4" library="0jlib" package="3DIGIT-7SEG" value="3DIGIT-7SEG"/>
<element name="R4-10" library="resistor" package="R0805" value="5.6"/>
<element name="R4-11" library="resistor" package="R0805" value="5.6"/>
<element name="R4-12" library="resistor" package="R0805" value="5.6"/>
<element name="R4-13" library="resistor" package="R0805" value="5.6"/>
<element name="R4-14" library="resistor" package="R0805" value="5.6"/>
<element name="R4-15" library="resistor" package="R0805" value="5.6"/>
<element name="R4-16" library="resistor" package="R0805" value="5.6"/>
<element name="R4-17" library="resistor" package="R0805" value="5.6"/>
<element name="F5-1" library="fuse" package="SH22,5" value="FUSESH22,5">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R0-3" library="resistor" package="R0805" value="10k"/>
<element name="R0-2" library="resistor" package="R0805" value="10k"/>
<element name="R6-1" library="resistor" package="R0805" value="68"/>
<element name="R6-2" library="resistor" package="R0805" value="5.6"/>
<element name="R6-3" library="resistor" package="R0805" value="8.2"/>
<element name="R6-7" library="resistor" package="R0805" value="68"/>
<element name="R6-8" library="resistor" package="R0805" value="5.6"/>
<element name="R6-9" library="resistor" package="R0805" value="8.2"/>
<element name="R6-4" library="resistor" package="R0805" value="68"/>
<element name="R6-5" library="resistor" package="R0805" value="5.6"/>
<element name="R6-6" library="resistor" package="R0805" value="8.2"/>
<element name="R6-10" library="resistor" package="R0805" value="68"/>
<element name="R6-11" library="resistor" package="R0805" value="5.6"/>
<element name="R6-12" library="resistor" package="R0805" value="8.2"/>
<element name="T0-1" library="transistor" package="SOT23" value="BC846"/>
<element name="R0-4" library="resistor" package="R0805" value="750"/>
<element name="R0-5" library="resistor" package="R0805" value="100k"/>
<element name="LCD" library="0jlib" package="EADOGL128S" value="EADOGL128"/>
<element name="R0-6" library="resistor" package="R0805" value="22"/>
<element name="R0-7" library="resistor" package="R0805" value="22"/>
<element name="R0-8" library="resistor" package="R0805" value="22"/>
<element name="C0-4" library="resistor" package="C0805" value="1u"/>
<element name="C0-5" library="resistor" package="C0805" value="1u"/>
<element name="C0-6" library="resistor" package="C0805" value="1u"/>
<element name="C0-7" library="resistor" package="C0805" value="1u"/>
<element name="C0-8" library="resistor" package="C0805" value="1u"/>
<element name="C0-9" library="resistor" package="C0805" value="1u"/>
<element name="C0-10" library="resistor" package="C0805" value="1u"/>
<element name="C0-11" library="resistor" package="C0805" value="1u"/>
<element name="C0-12" library="resistor" package="C0805" value="1u"/>
<element name="T0-2" library="transistor" package="SOT23" value="BC846"/>
<element name="R0-9" library="resistor" package="R0805" value="750"/>
<element name="R0-10" library="resistor" package="R0805" value="100k"/>
<element name="IC5-1" library="st-microelectronics" package="HSOP8" value="L5973D">
<attribute name="MPN" value="L5973D"/>
<attribute name="MF" value="STMICROELECTRONICS"/>
<attribute name="OC_FARNELL" value="1077145"/>
</element>
<element name="X5-1" library="con-cypressindustries" package="32005-201" value="MINI-USB-32005-201">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="R5-1" library="resistor" package="R0805" value="5.6k"/>
<element name="R5-2" library="resistor" package="R0805" value="3.3k"/>
<element name="R5-3" library="resistor" package="R0805" value="4.7k"/>
<element name="C5-1" library="resistor" package="C1206" value="10u"/>
<element name="C5-2" library="resistor" package="SMC_D" value="330u"/>
<element name="C5-3" library="resistor" package="C1206" value="220p"/>
<element name="C5-4" library="resistor" package="C1206" value="22n"/>
<element name="D5-2" library="diode" package="SMB" value=""/>
<element name="L5-1" library="inductor-coilcraft" package="DO3316P" value="15u">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="D5-1" library="diode" package="SMBG" value=""/>
<element name="T6-1" library="transistor" package="SOT23" value="BC846"/>
<element name="R6-13" library="resistor" package="R0805" value="750"/>
<element name="R6-14" library="resistor" package="R0805" value="100k"/>
<element name="T6-2" library="transistor" package="SOT23" value="BC846"/>
<element name="R6-15" library="resistor" package="R0805" value="750"/>
<element name="R6-16" library="resistor" package="R0805" value="100k"/>
<element name="T6-3" library="transistor" package="SOT23" value="BC846"/>
<element name="R6-17" library="resistor" package="R0805" value="750"/>
<element name="R6-18" library="resistor" package="R0805" value="100k"/>
<element name="C5-5" library="resistor" package="C0805" value="100n"/>
<element name="SG0-1" library="buzzer" package="F/CM12P" value="F/CM12P">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
</element>
<element name="C0-2" library="resistor" package="C0805" value="100n"/>
<element name="C0-3" library="resistor" package="C0805" value="100n"/>
<element name="C0-14" library="resistor" package="C0805" value="100n"/>
<element name="JP0-2" library="pinhead" package="2X03" value=""/>
<element name="R0-11" library="resistor" package="R0805" value="10k"/>
<element name="D6_1" library="0jlib" package="LED_RGB_PLCC6" value="LED_RGB_PLCC6"/>
<element name="D6-2" library="0jlib" package="LED_RGB_PLCC6" value="LED_RGB_PLCC6"/>
<element name="D6-3" library="0jlib" package="LED_RGB_PLCC6" value="LED_RGB_PLCC6"/>
<element name="D6-4" library="0jlib" package="LED_RGB_PLCC6" value="LED_RGB_PLCC6"/>
<element name="R6-19" library="resistor" package="R0805" value="68"/>
<element name="R6-20" library="resistor" package="R0805" value="5.6"/>
<element name="R6-21" library="resistor" package="R0805" value="8.2"/>
<element name="R6-22" library="resistor" package="R0805" value="68"/>
<element name="R6-23" library="resistor" package="R0805" value="5.6"/>
<element name="R6-24" library="resistor" package="R0805" value="8.2"/>
<element name="R6-25" library="resistor" package="R0805" value="68"/>
<element name="R6-26" library="resistor" package="R0805" value="5.6"/>
<element name="R6-27" library="resistor" package="R0805" value="8.2"/>
<element name="R6-28" library="resistor" package="R0805" value="68"/>
<element name="R6-29" library="resistor" package="R0805" value="5.6"/>
<element name="R6-30" library="resistor" package="R0805" value="8.2"/>
<element name="D6-5" library="0jlib" package="LED_RGB_PLCC6" value="LED_RGB_PLCC6"/>
<element name="D6-6" library="0jlib" package="LED_RGB_PLCC6" value="LED_RGB_PLCC6"/>
<element name="D6-7" library="0jlib" package="LED_RGB_PLCC6" value="LED_RGB_PLCC6"/>
<element name="D6-8" library="0jlib" package="LED_RGB_PLCC6" value="LED_RGB_PLCC6"/>
<element name="T6-4" library="transistor" package="SOT23" value="BC846"/>
<element name="R6-31" library="resistor" package="R0805" value="750"/>
<element name="R6-32" library="resistor" package="R0805" value="100k"/>
<element name="T6-5" library="transistor" package="SOT23" value="BC846"/>
<element name="R6-33" library="resistor" package="R0805" value="750"/>
<element name="R6-34" library="resistor" package="R0805" value="100k"/>
<element name="T6-6" library="transistor" package="SOT23" value="BC846"/>
<element name="R6-35" library="resistor" package="R0805" value="750"/>
<element name="R6-36" library="resistor" package="R0805" value="100k"/>
<element name="LED1-5" library="led" package="CHIPLED_0805" value=""/>
<element name="LED1-6" library="led" package="CHIPLED_0805" value=""/>
<element name="R1-18" library="resistor" package="R0805" value="4.7"/>
<element name="R1-19" library="resistor" package="R0805" value="4.7"/>
<element name="U$1" library="avr-7" package="TQFP44" value="XMEGA-A4TQFP"/>
<element name="JP1" library="pinhead" package="1X04" value=""/>
<element name="R2-18" library="resistor" package="R0805" value="4.7"/>
<element name="R2-19" library="resistor" package="R0805" value="4.7"/>
<element name="LED2-5" library="led" package="CHIPLED_0805" value=""/>
<element name="LED2-6" library="led" package="CHIPLED_0805" value=""/>
<element name="R3-18" library="resistor" package="R0805" value="4.7"/>
<element name="R3-19" library="resistor" package="R0805" value="4.7"/>
<element name="LED3-5" library="led" package="CHIPLED_0805" value=""/>
<element name="LED3-6" library="led" package="CHIPLED_0805" value=""/>
<element name="R4-18" library="resistor" package="R0805" value="4.7"/>
<element name="R4-19" library="resistor" package="R0805" value="4.7"/>
<element name="LED4-5" library="led" package="CHIPLED_0805" value=""/>
<element name="LED4-6" library="led" package="CHIPLED_0805" value=""/>
<element name="C0-1" library="resistor" package="C0805" value="100n"/>
</elements>
<signals>
<signal name="VCC">
<contactref element="R0-1" pad="2"/>
<contactref element="R1-1" pad="2"/>
<contactref element="IC1-1" pad="6"/>
<contactref element="IC1-1" pad="4"/>
<contactref element="C1-1" pad="1"/>
<contactref element="JP1-1" pad="2"/>
<contactref element="R1-2" pad="2"/>
<contactref element="R1-3" pad="2"/>
<contactref element="IC2-1" pad="4"/>
<contactref element="IC2-1" pad="6"/>
<contactref element="R2-1" pad="2"/>
<contactref element="C2-1" pad="1"/>
<contactref element="JP2-1" pad="2"/>
<contactref element="R2-2" pad="2"/>
<contactref element="R2-3" pad="2"/>
<contactref element="R2-6" pad="2"/>
<contactref element="R2-9" pad="2"/>
<contactref element="R2-8" pad="2"/>
<contactref element="R2-7" pad="2"/>
<contactref element="IC3-1" pad="4"/>
<contactref element="IC3-1" pad="6"/>
<contactref element="R3-1" pad="2"/>
<contactref element="C3-1" pad="1"/>
<contactref element="JP3-1" pad="2"/>
<contactref element="R3-2" pad="2"/>
<contactref element="R3-3" pad="2"/>
<contactref element="R3-6" pad="2"/>
<contactref element="R3-9" pad="2"/>
<contactref element="R3-8" pad="2"/>
<contactref element="R3-7" pad="2"/>
<contactref element="IC4-1" pad="4"/>
<contactref element="IC4-1" pad="6"/>
<contactref element="R4-1" pad="2"/>
<contactref element="C4-1" pad="1"/>
<contactref element="JP4-1" pad="2"/>
<contactref element="R4-2" pad="2"/>
<contactref element="R4-3" pad="2"/>
<contactref element="R4-6" pad="2"/>
<contactref element="R4-9" pad="2"/>
<contactref element="R4-8" pad="2"/>
<contactref element="R4-7" pad="2"/>
<contactref element="IC2-1" pad="1"/>
<contactref element="IC3-1" pad="2"/>
<contactref element="IC4-1" pad="1"/>
<contactref element="IC4-1" pad="2"/>
<contactref element="IC1-1" pad="18"/>
<contactref element="IC2-1" pad="18"/>
<contactref element="IC4-1" pad="18"/>
<contactref element="IC3-1" pad="18"/>
<contactref element="R0-3" pad="2"/>
<contactref element="LCD" pad="LCD_P35"/>
<contactref element="LCD" pad="LCD_P34"/>
<contactref element="R0-8" pad="2"/>
<contactref element="R0-7" pad="2"/>
<contactref element="R0-6" pad="2"/>
<contactref element="R0-2" pad="2"/>
<contactref element="R5-1" pad="2"/>
<contactref element="C5-2" pad="+"/>
<contactref element="L5-1" pad="2"/>
<contactref element="C5-5" pad="1"/>
<contactref element="SG0-1" pad="-"/>
<contactref element="D6_1" pad="3"/>
<contactref element="D6_1" pad="2"/>
<contactref element="D6_1" pad="1"/>
<contactref element="D6-2" pad="3"/>
<contactref element="D6-2" pad="2"/>
<contactref element="D6-2" pad="1"/>
<contactref element="D6-3" pad="1"/>
<contactref element="D6-3" pad="2"/>
<contactref element="D6-3" pad="3"/>
<contactref element="D6-4" pad="1"/>
<contactref element="D6-4" pad="2"/>
<contactref element="D6-4" pad="3"/>
<contactref element="D6-7" pad="1"/>
<contactref element="D6-7" pad="2"/>
<contactref element="D6-7" pad="3"/>
<contactref element="D6-5" pad="3"/>
<contactref element="D6-5" pad="2"/>
<contactref element="D6-5" pad="1"/>
<contactref element="D6-6" pad="3"/>
<contactref element="D6-6" pad="2"/>
<contactref element="D6-6" pad="1"/>
<contactref element="D6-8" pad="1"/>
<contactref element="D6-8" pad="2"/>
<contactref element="D6-8" pad="3"/>
<contactref element="U$1" pad="9"/>
<contactref element="U$1" pad="19"/>
<contactref element="U$1" pad="31"/>
<contactref element="C0-3" pad="2"/>
<contactref element="C0-14" pad="2"/>
<contactref element="C0-2" pad="2"/>
<contactref element="JP1" pad="1"/>
<contactref element="JP0-2" pad="2"/>
<contactref element="R2-19" pad="2"/>
<contactref element="R2-18" pad="2"/>
<contactref element="R1-9" pad="2"/>
<contactref element="R1-18" pad="2"/>
<contactref element="R1-8" pad="2"/>
<contactref element="R1-7" pad="2"/>
<contactref element="R1-6" pad="2"/>
<contactref element="R1-19" pad="2"/>
<contactref element="R3-18" pad="2"/>
<contactref element="R3-19" pad="2"/>
<contactref element="R4-19" pad="2"/>
<contactref element="R4-18" pad="2"/>
<contactref element="C0-1" pad="2"/>
</signal>
<signal name="GND">
<contactref element="IC1-1" pad="3"/>
<contactref element="IC1-1" pad="5"/>
<contactref element="C1-3" pad="1"/>
<contactref element="C1-2" pad="1"/>
<contactref element="C1-1" pad="2"/>
<contactref element="JP1-1" pad="6"/>
<contactref element="T1-1" pad="2"/>
<contactref element="R1-5" pad="1"/>
<contactref element="IC2-1" pad="3"/>
<contactref element="IC2-1" pad="5"/>
<contactref element="C2-3" pad="1"/>
<contactref element="C2-2" pad="1"/>
<contactref element="C2-1" pad="2"/>
<contactref element="JP2-1" pad="6"/>
<contactref element="T2-1" pad="2"/>
<contactref element="R2-5" pad="1"/>
<contactref element="IC3-1" pad="3"/>
<contactref element="IC3-1" pad="5"/>
<contactref element="C3-3" pad="1"/>
<contactref element="C3-2" pad="1"/>
<contactref element="C3-1" pad="2"/>
<contactref element="JP3-1" pad="6"/>
<contactref element="T3-1" pad="2"/>
<contactref element="R3-5" pad="1"/>
<contactref element="IC2-1" pad="2"/>
<contactref element="IC4-1" pad="3"/>
<contactref element="IC4-1" pad="5"/>
<contactref element="C4-3" pad="1"/>
<contactref element="C4-2" pad="1"/>
<contactref element="C4-1" pad="2"/>
<contactref element="JP4-1" pad="6"/>
<contactref element="T4-1" pad="2"/>
<contactref element="R4-5" pad="1"/>
<contactref element="IC1-1" pad="1"/>
<contactref element="IC1-1" pad="2"/>
<contactref element="IC3-1" pad="1"/>
<contactref element="IC1-1" pad="21"/>
<contactref element="IC2-1" pad="21"/>
<contactref element="IC4-1" pad="21"/>
<contactref element="IC3-1" pad="21"/>
<contactref element="R0-5" pad="1"/>
<contactref element="T0-1" pad="2"/>
<contactref element="C0-4" pad="1"/>
<contactref element="C0-5" pad="1"/>
<contactref element="C0-6" pad="1"/>
<contactref element="C0-7" pad="1"/>
<contactref element="C0-8" pad="1"/>
<contactref element="C0-9" pad="1"/>
<contactref element="LCD" pad="LCD_P26"/>
<contactref element="LCD" pad="LCD_P33"/>
<contactref element="T0-2" pad="2"/>
<contactref element="R0-10" pad="1"/>
<contactref element="IC5-1" pad="7"/>
<contactref element="X5-1" pad="5"/>
<contactref element="R5-2" pad="1"/>
<contactref element="R5-3" pad="1"/>
<contactref element="IC5-1" pad="3"/>
<contactref element="C5-1" pad="2"/>
<contactref element="C5-2" pad="-"/>
<contactref element="C5-3" pad="2"/>
<contactref element="D5-2" pad="A"/>
<contactref element="D5-1" pad="A"/>
<contactref element="T6-1" pad="2"/>
<contactref element="R6-14" pad="1"/>
<contactref element="T6-2" pad="2"/>
<contactref element="R6-16" pad="1"/>
<contactref element="T6-3" pad="2"/>
<contactref element="R6-18" pad="1"/>
<contactref element="C5-5" pad="2"/>
<contactref element="C0-3" pad="1"/>
<contactref element="C0-14" pad="1"/>
<contactref element="JP0-2" pad="6"/>
<contactref element="R0-11" pad="1"/>
<contactref element="C0-2" pad="1"/>
<contactref element="T6-4" pad="2"/>
<contactref element="R6-32" pad="1"/>
<contactref element="T6-5" pad="2"/>
<contactref element="R6-34" pad="1"/>
<contactref element="T6-6" pad="2"/>
<contactref element="R6-36" pad="1"/>
<contactref element="U$1" pad="38"/>
<contactref element="U$1" pad="8"/>
<contactref element="U$1" pad="18"/>
<contactref element="U$1" pad="30"/>
<contactref element="JP1" pad="4"/>
<contactref element="C0-1" pad="1"/>
</signal>
<signal name="1-MOSI">
<contactref element="IC1-1" pad="15"/>
<contactref element="JP1-1" pad="4"/>
</signal>
<signal name="1-MISO">
<contactref element="IC1-1" pad="16"/>
<contactref element="JP1-1" pad="1"/>
</signal>
<signal name="1-SCK">
<contactref element="IC1-1" pad="17"/>
<contactref element="JP1-1" pad="3"/>
</signal>
<signal name="SDA">
<contactref element="IC1-1" pad="27"/>
<contactref element="R1-3" pad="1"/>
<contactref element="IC2-1" pad="27"/>
<contactref element="R2-3" pad="1"/>
<contactref element="IC3-1" pad="27"/>
<contactref element="R3-3" pad="1"/>
<contactref element="IC4-1" pad="27"/>
<contactref element="R4-3" pad="1"/>
<contactref element="R0-3" pad="1"/>
<contactref element="U$1" pad="10"/>
</signal>
<signal name="SCL">
<contactref element="IC1-1" pad="28"/>
<contactref element="R1-2" pad="1"/>
<contactref element="IC2-1" pad="28"/>
<contactref element="R2-2" pad="1"/>
<contactref element="IC3-1" pad="28"/>
<contactref element="R3-2" pad="1"/>
<contactref element="IC4-1" pad="28"/>
<contactref element="R4-2" pad="1"/>
<contactref element="R0-2" pad="1"/>
<contactref element="U$1" pad="11"/>
</signal>
<signal name="N$10">
<contactref element="R1-4" pad="1"/>
<contactref element="IC1-1" pad="24"/>
</signal>
<signal name="N$11">
<contactref element="R1-4" pad="2"/>
<contactref element="T1-1" pad="1"/>
<contactref element="R1-5" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="T1-1" pad="3"/>
<contactref element="LED1-4" pad="C"/>
<contactref element="LED1-3" pad="C"/>
<contactref element="LED1-2" pad="C"/>
<contactref element="LED1-1" pad="C"/>
<contactref element="LED1-5" pad="C"/>
<contactref element="LED1-6" pad="C"/>
</signal>
<signal name="N$13">
<contactref element="LED1-1" pad="A"/>
<contactref element="R1-6" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="LED1-2" pad="A"/>
<contactref element="R1-7" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="LED1-3" pad="A"/>
<contactref element="R1-8" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="LED1-4" pad="A"/>
<contactref element="R1-9" pad="1"/>
</signal>
<signal name="7SEG1-5">
<contactref element="IC1-1" pad="25"/>
<contactref element="R1-14" pad="2"/>
</signal>
<signal name="7SEG1-4">
<contactref element="IC1-1" pad="26"/>
<contactref element="R1-13" pad="2"/>
</signal>
<signal name="7SEG1-3">
<contactref element="IC1-1" pad="30"/>
<contactref element="R1-12" pad="2"/>
</signal>
<signal name="7SEG1-2">
<contactref element="IC1-1" pad="31"/>
<contactref element="R1-11" pad="2"/>
</signal>
<signal name="7SEG1-1">
<contactref element="IC1-1" pad="32"/>
<contactref element="R1-10" pad="2"/>
</signal>
<signal name="7SEG1-10">
<contactref element="R1-16" pad="2"/>
<contactref element="IC1-1" pad="12"/>
</signal>
<signal name="7SEG1-9">
<contactref element="7SEG1" pad="9"/>
<contactref element="IC1-1" pad="11"/>
</signal>
<signal name="7SEG1-8">
<contactref element="7SEG1" pad="8"/>
<contactref element="IC1-1" pad="10"/>
</signal>
<signal name="7SEG1-7">
<contactref element="R1-15" pad="2"/>
<contactref element="IC1-1" pad="9"/>
</signal>
<signal name="7SEG1-12">
<contactref element="7SEG1" pad="12"/>
<contactref element="IC1-1" pad="14"/>
</signal>
<signal name="7SEG1-11">
<contactref element="R1-17" pad="2"/>
<contactref element="IC1-1" pad="13"/>
</signal>
<signal name="N$9">
<contactref element="R1-10" pad="1"/>
<contactref element="7SEG1" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="7SEG1" pad="2"/>
<contactref element="R1-11" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="R1-12" pad="1"/>
<contactref element="7SEG1" pad="3"/>
</signal>
<signal name="N$19">
<contactref element="7SEG1" pad="4"/>
<contactref element="R1-13" pad="1"/>
</signal>
<signal name="N$20">
<contactref element="R1-14" pad="1"/>
<contactref element="7SEG1" pad="5"/>
</signal>
<signal name="N$21">
<contactref element="7SEG1" pad="7"/>
<contactref element="R1-15" pad="1"/>
</signal>
<signal name="N$24">
<contactref element="R1-16" pad="1"/>
<contactref element="7SEG1" pad="10"/>
</signal>
<signal name="N$25">
<contactref element="7SEG1" pad="11"/>
<contactref element="R1-17" pad="1"/>
</signal>
<signal name="1-XTAL2">
<contactref element="IC1-1" pad="8"/>
<contactref element="C1-2" pad="2"/>
<contactref element="Q1-1" pad="1"/>
</signal>
<signal name="2-MOSI">
<contactref element="IC2-1" pad="15"/>
<contactref element="JP2-1" pad="4"/>
</signal>
<signal name="2-MISO">
<contactref element="IC2-1" pad="16"/>
<contactref element="JP2-1" pad="1"/>
</signal>
<signal name="2-SCK">
<contactref element="IC2-1" pad="17"/>
<contactref element="JP2-1" pad="3"/>
</signal>
<signal name="N$29">
<contactref element="R2-4" pad="1"/>
<contactref element="IC2-1" pad="24"/>
</signal>
<signal name="N$30">
<contactref element="R2-4" pad="2"/>
<contactref element="T2-1" pad="1"/>
<contactref element="R2-5" pad="2"/>
</signal>
<signal name="N$31">
<contactref element="T2-1" pad="3"/>
<contactref element="LED2-4" pad="C"/>
<contactref element="LED2-3" pad="C"/>
<contactref element="LED2-2" pad="C"/>
<contactref element="LED2-1" pad="C"/>
<contactref element="LED2-5" pad="C"/>
<contactref element="LED2-6" pad="C"/>
</signal>
<signal name="N$32">
<contactref element="LED2-1" pad="A"/>
<contactref element="R2-6" pad="1"/>
</signal>
<signal name="N$33">
<contactref element="LED2-2" pad="A"/>
<contactref element="R2-7" pad="1"/>
</signal>
<signal name="N$34">
<contactref element="LED2-3" pad="A"/>
<contactref element="R2-8" pad="1"/>
</signal>
<signal name="N$35">
<contactref element="LED2-4" pad="A"/>
<contactref element="R2-9" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="R2-10" pad="1"/>
<contactref element="7SEG2" pad="1"/>
</signal>
<signal name="N$37">
<contactref element="7SEG2" pad="2"/>
<contactref element="R2-11" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="R2-12" pad="1"/>
<contactref element="7SEG2" pad="3"/>
</signal>
<signal name="N$39">
<contactref element="7SEG2" pad="4"/>
<contactref element="R2-13" pad="1"/>
</signal>
<signal name="N$40">
<contactref element="R2-14" pad="1"/>
<contactref element="7SEG2" pad="5"/>
</signal>
<signal name="N$41">
<contactref element="7SEG2" pad="7"/>
<contactref element="R2-15" pad="1"/>
</signal>
<signal name="N$44">
<contactref element="R2-16" pad="1"/>
<contactref element="7SEG2" pad="10"/>
</signal>
<signal name="N$45">
<contactref element="7SEG2" pad="11"/>
<contactref element="R2-17" pad="1"/>
</signal>
<signal name="2-XTAL1">
<contactref element="IC2-1" pad="7"/>
<contactref element="C2-3" pad="2"/>
<contactref element="Q2-1" pad="2"/>
</signal>
<signal name="2-XTAL2">
<contactref element="IC2-1" pad="8"/>
<contactref element="C2-2" pad="2"/>
<contactref element="Q2-1" pad="1"/>
</signal>
<signal name="KP_ROW1">
<contactref element="KEYPAD" pad="5/ROW1"/>
<contactref element="U$1" pad="43"/>
</signal>
<signal name="KP_ROW2">
<contactref element="KEYPAD" pad="6/ROW2"/>
<contactref element="U$1" pad="42"/>
</signal>
<signal name="KP_ROW3">
<contactref element="KEYPAD" pad="7/ROW3"/>
<contactref element="U$1" pad="41"/>
</signal>
<signal name="KP_ROW4">
<contactref element="KEYPAD" pad="8/ROW4"/>
<contactref element="U$1" pad="40"/>
</signal>
<signal name="KP_COL1">
<contactref element="KEYPAD" pad="1/COL1"/>
<contactref element="U$1" pad="3"/>
</signal>
<signal name="KP_COL2">
<contactref element="KEYPAD" pad="2/COL2"/>
<contactref element="U$1" pad="2"/>
</signal>
<signal name="KP_COL3">
<contactref element="KEYPAD" pad="3/COL3"/>
<contactref element="U$1" pad="1"/>
</signal>
<signal name="KP_COL4">
<contactref element="KEYPAD" pad="4/COL4"/>
<contactref element="U$1" pad="44"/>
</signal>
<signal name="3-MOSI">
<contactref element="IC3-1" pad="15"/>
<contactref element="JP3-1" pad="4"/>
</signal>
<signal name="3-MISO">
<contactref element="IC3-1" pad="16"/>
<contactref element="JP3-1" pad="1"/>
</signal>
<signal name="3-SCK">
<contactref element="IC3-1" pad="17"/>
<contactref element="JP3-1" pad="3"/>
</signal>
<signal name="N$58">
<contactref element="R3-4" pad="1"/>
<contactref element="IC3-1" pad="24"/>
</signal>
<signal name="N$59">
<contactref element="R3-4" pad="2"/>
<contactref element="T3-1" pad="1"/>
<contactref element="R3-5" pad="2"/>
</signal>
<signal name="N$60">
<contactref element="T3-1" pad="3"/>
<contactref element="LED3-4" pad="C"/>
<contactref element="LED3-3" pad="C"/>
<contactref element="LED3-2" pad="C"/>
<contactref element="LED3-1" pad="C"/>
<contactref element="LED3-5" pad="C"/>
<contactref element="LED3-6" pad="C"/>
</signal>
<signal name="N$61">
<contactref element="LED3-1" pad="A"/>
<contactref element="R3-6" pad="1"/>
</signal>
<signal name="N$62">
<contactref element="LED3-2" pad="A"/>
<contactref element="R3-7" pad="1"/>
</signal>
<signal name="N$63">
<contactref element="LED3-3" pad="A"/>
<contactref element="R3-8" pad="1"/>
</signal>
<signal name="N$66">
<contactref element="LED3-4" pad="A"/>
<contactref element="R3-9" pad="1"/>
</signal>
<signal name="N$67">
<contactref element="R3-10" pad="1"/>
<contactref element="7SEG3" pad="1"/>
</signal>
<signal name="N$68">
<contactref element="7SEG3" pad="2"/>
<contactref element="R3-11" pad="1"/>
</signal>
<signal name="N$69">
<contactref element="R3-12" pad="1"/>
<contactref element="7SEG3" pad="3"/>
</signal>
<signal name="N$70">
<contactref element="7SEG3" pad="4"/>
<contactref element="R3-13" pad="1"/>
</signal>
<signal name="N$71">
<contactref element="R3-14" pad="1"/>
<contactref element="7SEG3" pad="5"/>
</signal>
<signal name="N$72">
<contactref element="7SEG3" pad="7"/>
<contactref element="R3-15" pad="1"/>
</signal>
<signal name="N$75">
<contactref element="R3-16" pad="1"/>
<contactref element="7SEG3" pad="10"/>
</signal>
<signal name="N$76">
<contactref element="7SEG3" pad="11"/>
<contactref element="R3-17" pad="1"/>
</signal>
<signal name="3-XTAL1">
<contactref element="IC3-1" pad="7"/>
<contactref element="C3-3" pad="2"/>
<contactref element="Q3-1" pad="2"/>
</signal>
<signal name="3-XTAL2">
<contactref element="IC3-1" pad="8"/>
<contactref element="C3-2" pad="2"/>
<contactref element="Q3-1" pad="1"/>
</signal>
<signal name="7SEG2-1">
<contactref element="R2-10" pad="2"/>
<contactref element="IC2-1" pad="32"/>
</signal>
<signal name="7SEG3-2">
<contactref element="IC3-1" pad="31"/>
<contactref element="R3-11" pad="2"/>
</signal>
<signal name="7SEG2-3">
<contactref element="R2-12" pad="2"/>
<contactref element="IC2-1" pad="30"/>
</signal>
<signal name="7SEG2-2">
<contactref element="R2-11" pad="2"/>
<contactref element="IC2-1" pad="31"/>
</signal>
<signal name="7SEG2-4">
<contactref element="R2-13" pad="2"/>
<contactref element="IC2-1" pad="26"/>
</signal>
<signal name="7SEG2-5">
<contactref element="R2-14" pad="2"/>
<contactref element="IC2-1" pad="25"/>
</signal>
<signal name="7SEG2-7">
<contactref element="R2-15" pad="2"/>
<contactref element="IC2-1" pad="9"/>
</signal>
<signal name="7SEG2-8">
<contactref element="7SEG2" pad="8"/>
<contactref element="IC2-1" pad="10"/>
</signal>
<signal name="7SEG2-9">
<contactref element="7SEG2" pad="9"/>
<contactref element="IC2-1" pad="11"/>
</signal>
<signal name="7SEG2-10">
<contactref element="R2-16" pad="2"/>
<contactref element="IC2-1" pad="12"/>
</signal>
<signal name="7SEG2-11">
<contactref element="R2-17" pad="2"/>
<contactref element="IC2-1" pad="13"/>
</signal>
<signal name="7SEG2-12">
<contactref element="7SEG2" pad="12"/>
<contactref element="IC2-1" pad="14"/>
</signal>
<signal name="2-!RESET">
<contactref element="JP2-1" pad="5"/>
<contactref element="IC2-1" pad="29"/>
<contactref element="R2-1" pad="1"/>
</signal>
<signal name="1-!RESET">
<contactref element="IC1-1" pad="29"/>
<contactref element="JP1-1" pad="5"/>
<contactref element="R1-1" pad="1"/>
</signal>
<signal name="0-!RESET">
<contactref element="R0-1" pad="1"/>
<contactref element="JP0-2" pad="5"/>
<contactref element="U$1" pad="35"/>
</signal>
<signal name="3-!RESET">
<contactref element="IC3-1" pad="29"/>
<contactref element="R3-1" pad="1"/>
<contactref element="JP3-1" pad="5"/>
</signal>
<signal name="7SEG3-1">
<contactref element="R3-10" pad="2"/>
<contactref element="IC3-1" pad="32"/>
</signal>
<signal name="7SEG3-3">
<contactref element="IC3-1" pad="30"/>
<contactref element="R3-12" pad="2"/>
</signal>
<signal name="7SEG3-4">
<contactref element="IC3-1" pad="26"/>
<contactref element="R3-13" pad="2"/>
</signal>
<signal name="7SEG3-5">
<contactref element="IC3-1" pad="25"/>
<contactref element="R3-14" pad="2"/>
</signal>
<signal name="7SEG3-7">
<contactref element="R3-15" pad="2"/>
<contactref element="IC3-1" pad="9"/>
</signal>
<signal name="7SEG3-8">
<contactref element="7SEG3" pad="8"/>
<contactref element="IC3-1" pad="10"/>
</signal>
<signal name="7SEG3-9">
<contactref element="7SEG3" pad="9"/>
<contactref element="IC3-1" pad="11"/>
</signal>
<signal name="7SEG3-10">
<contactref element="R3-16" pad="2"/>
<contactref element="IC3-1" pad="12"/>
</signal>
<signal name="7SEG3-11">
<contactref element="R3-17" pad="2"/>
<contactref element="IC3-1" pad="13"/>
</signal>
<signal name="7SEG3-12">
<contactref element="7SEG3" pad="12"/>
<contactref element="IC3-1" pad="14"/>
</signal>
<signal name="4-MOSI">
<contactref element="IC4-1" pad="15"/>
<contactref element="JP4-1" pad="4"/>
</signal>
<signal name="4-MISO">
<contactref element="IC4-1" pad="16"/>
<contactref element="JP4-1" pad="1"/>
</signal>
<signal name="4-SCK">
<contactref element="IC4-1" pad="17"/>
<contactref element="JP4-1" pad="3"/>
</signal>
<signal name="N$84">
<contactref element="R4-4" pad="1"/>
<contactref element="IC4-1" pad="24"/>
</signal>
<signal name="N$85">
<contactref element="R4-4" pad="2"/>
<contactref element="T4-1" pad="1"/>
<contactref element="R4-5" pad="2"/>
</signal>
<signal name="N$86">
<contactref element="T4-1" pad="3"/>
<contactref element="LED4-4" pad="C"/>
<contactref element="LED4-3" pad="C"/>
<contactref element="LED4-2" pad="C"/>
<contactref element="LED4-1" pad="C"/>
<contactref element="LED4-6" pad="C"/>
<contactref element="LED4-5" pad="C"/>
</signal>
<signal name="N$87">
<contactref element="LED4-1" pad="A"/>
<contactref element="R4-6" pad="1"/>
</signal>
<signal name="N$88">
<contactref element="LED4-2" pad="A"/>
<contactref element="R4-7" pad="1"/>
</signal>
<signal name="N$89">
<contactref element="LED4-3" pad="A"/>
<contactref element="R4-8" pad="1"/>
</signal>
<signal name="N$90">
<contactref element="LED4-4" pad="A"/>
<contactref element="R4-9" pad="1"/>
</signal>
<signal name="N$91">
<contactref element="R4-10" pad="1"/>
<contactref element="7SEG4" pad="1"/>
</signal>
<signal name="N$92">
<contactref element="7SEG4" pad="2"/>
<contactref element="R4-11" pad="1"/>
</signal>
<signal name="N$93">
<contactref element="R4-12" pad="1"/>
<contactref element="7SEG4" pad="3"/>
</signal>
<signal name="N$94">
<contactref element="7SEG4" pad="4"/>
<contactref element="R4-13" pad="1"/>
</signal>
<signal name="N$95">
<contactref element="R4-14" pad="1"/>
<contactref element="7SEG4" pad="5"/>
</signal>
<signal name="N$96">
<contactref element="7SEG4" pad="7"/>
<contactref element="R4-15" pad="1"/>
</signal>
<signal name="N$99">
<contactref element="R4-16" pad="1"/>
<contactref element="7SEG4" pad="10"/>
</signal>
<signal name="N$100">
<contactref element="7SEG4" pad="11"/>
<contactref element="R4-17" pad="1"/>
</signal>
<signal name="4-XTAL1">
<contactref element="IC4-1" pad="7"/>
<contactref element="C4-3" pad="2"/>
<contactref element="Q4-1" pad="2"/>
</signal>
<signal name="4-XTAL2">
<contactref element="IC4-1" pad="8"/>
<contactref element="C4-2" pad="2"/>
<contactref element="Q4-1" pad="1"/>
</signal>
<signal name="4-!RESET">
<contactref element="JP4-1" pad="5"/>
<contactref element="IC4-1" pad="29"/>
<contactref element="R4-1" pad="1"/>
</signal>
<signal name="7SEG4-1">
<contactref element="IC4-1" pad="32"/>
<contactref element="R4-10" pad="2"/>
</signal>
<signal name="7SEG4-2">
<contactref element="R4-11" pad="2"/>
<contactref element="IC4-1" pad="31"/>
</signal>
<signal name="7SEG4-3">
<contactref element="R4-12" pad="2"/>
<contactref element="IC4-1" pad="30"/>
</signal>
<signal name="7SEG4-4">
<contactref element="R4-13" pad="2"/>
<contactref element="IC4-1" pad="26"/>
</signal>
<signal name="7SEG4-5">
<contactref element="R4-14" pad="2"/>
<contactref element="IC4-1" pad="25"/>
</signal>
<signal name="7SEG4-7">
<contactref element="R4-15" pad="2"/>
<contactref element="IC4-1" pad="9"/>
</signal>
<signal name="7SEG4-8">
<contactref element="7SEG4" pad="8"/>
<contactref element="IC4-1" pad="10"/>
</signal>
<signal name="7SEG4-9">
<contactref element="7SEG4" pad="9"/>
<contactref element="IC4-1" pad="11"/>
</signal>
<signal name="7SEG4-10">
<contactref element="R4-16" pad="2"/>
<contactref element="IC4-1" pad="12"/>
</signal>
<signal name="7SEG4-11">
<contactref element="R4-17" pad="2"/>
<contactref element="IC4-1" pad="13"/>
</signal>
<signal name="7SEG4-12">
<contactref element="7SEG4" pad="12"/>
<contactref element="IC4-1" pad="14"/>
</signal>
<signal name="N$54">
<contactref element="F5-1" pad="1"/>
<contactref element="X5-1" pad="1"/>
</signal>
<signal name="N$105">
</signal>
<signal name="N$106">
</signal>
<signal name="N$107">
</signal>
<signal name="N$108">
</signal>
<signal name="LOGO_BLUE">
<contactref element="T6-3" pad="3"/>
<contactref element="R6-1" pad="2"/>
<contactref element="R6-7" pad="1"/>
<contactref element="R6-4" pad="1"/>
<contactref element="R6-10" pad="1"/>
</signal>
<signal name="1-XTAL1">
<contactref element="Q1-1" pad="2"/>
<contactref element="C1-3" pad="2"/>
<contactref element="IC1-1" pad="7"/>
</signal>
<signal name="LOGO_RED">
<contactref element="T6-1" pad="3"/>
<contactref element="R6-2" pad="1"/>
<contactref element="R6-8" pad="1"/>
<contactref element="R6-5" pad="1"/>
<contactref element="R6-11" pad="1"/>
</signal>
<signal name="LOGO_GREEN">
<contactref element="T6-2" pad="3"/>
<contactref element="R6-3" pad="1"/>
<contactref element="R6-9" pad="1"/>
<contactref element="R6-6" pad="1"/>
<contactref element="R6-12" pad="2"/>
</signal>
<signal name="BUZZER">
<contactref element="R0-4" pad="1"/>
<contactref element="U$1" pad="25"/>
</signal>
<signal name="N$6">
<contactref element="R0-4" pad="2"/>
<contactref element="T0-1" pad="1"/>
<contactref element="R0-5" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="T0-1" pad="3"/>
<contactref element="SG0-1" pad="+"/>
</signal>
<signal name="N$42">
<contactref element="R0-6" pad="1"/>
<contactref element="LCD" pad="LCD_P1"/>
</signal>
<signal name="N$46">
<contactref element="R0-7" pad="1"/>
<contactref element="LCD" pad="LCD_P2"/>
</signal>
<signal name="N$48">
<contactref element="R0-8" pad="1"/>
<contactref element="LCD" pad="LCD_P3"/>
</signal>
<signal name="N$51">
<contactref element="C0-4" pad="2"/>
<contactref element="LCD" pad="LCD_P32"/>
</signal>
<signal name="N$52">
<contactref element="LCD" pad="LCD_P25"/>
<contactref element="C0-5" pad="2"/>
</signal>
<signal name="N$55">
<contactref element="C0-6" pad="2"/>
<contactref element="LCD" pad="LCD_P24"/>
</signal>
<signal name="N$56">
<contactref element="LCD" pad="LCD_P23"/>
<contactref element="C0-7" pad="2"/>
</signal>
<signal name="N$57">
<contactref element="C0-8" pad="2"/>
<contactref element="LCD" pad="LCD_P22"/>
</signal>
<signal name="N$64">
<contactref element="LCD" pad="LCD_P21"/>
<contactref element="C0-9" pad="2"/>
</signal>
<signal name="N$65">
<contactref element="LCD" pad="LCD_P27"/>
<contactref element="C0-10" pad="2"/>
</signal>
<signal name="N$73">
<contactref element="C0-10" pad="1"/>
<contactref element="LCD" pad="LCD_P28"/>
</signal>
<signal name="N$74">
<contactref element="LCD" pad="LCD_P29"/>
<contactref element="C0-11" pad="2"/>
</signal>
<signal name="N$77">
<contactref element="LCD" pad="LCD_P30"/>
<contactref element="C0-11" pad="1"/>
<contactref element="C0-12" pad="2"/>
</signal>
<signal name="N$78">
<contactref element="LCD" pad="LCD_P31"/>
<contactref element="C0-12" pad="1"/>
</signal>
<signal name="LCD_A0">
<contactref element="LCD" pad="LCD_P38"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="LCD" pad="LCD_P18"/>
<contactref element="LCD" pad="LCD_P19"/>
<contactref element="LCD" pad="LCD_P20"/>
<contactref element="T0-2" pad="3"/>
</signal>
<signal name="N$49">
<contactref element="T0-2" pad="1"/>
<contactref element="R0-9" pad="2"/>
<contactref element="R0-10" pad="2"/>
</signal>
<signal name="LCD_LIGHT">
<contactref element="R0-9" pad="1"/>
<contactref element="U$1" pad="13"/>
</signal>
<signal name="N$79">
<contactref element="R5-1" pad="1"/>
<contactref element="R5-2" pad="2"/>
<contactref element="IC5-1" pad="5"/>
</signal>
<signal name="N$50">
<contactref element="F5-1" pad="2"/>
<contactref element="IC5-1" pad="8"/>
<contactref element="C5-1" pad="1"/>
<contactref element="D5-1" pad="C"/>
</signal>
<signal name="N$53">
<contactref element="IC5-1" pad="4"/>
<contactref element="C5-3" pad="1"/>
<contactref element="C5-4" pad="1"/>
</signal>
<signal name="N$97">
<contactref element="C5-4" pad="2"/>
<contactref element="R5-3" pad="2"/>
</signal>
<signal name="N$98">
<contactref element="D5-2" pad="C"/>
<contactref element="IC5-1" pad="1"/>
<contactref element="L5-1" pad="1"/>
</signal>
<signal name="N$82">
<contactref element="R6-13" pad="2"/>
<contactref element="T6-1" pad="1"/>
<contactref element="R6-14" pad="2"/>
</signal>
<signal name="N$83">
<contactref element="R6-15" pad="2"/>
<contactref element="T6-2" pad="1"/>
<contactref element="R6-16" pad="2"/>
</signal>
<signal name="N$101">
<contactref element="R6-17" pad="2"/>
<contactref element="T6-3" pad="1"/>
<contactref element="R6-18" pad="2"/>
</signal>
<signal name="LOGO_RED_CTRL">
<contactref element="R6-13" pad="1"/>
<contactref element="U$1" pad="21"/>
</signal>
<signal name="LOGO_GREEN_CTRL">
<contactref element="R6-15" pad="1"/>
<contactref element="U$1" pad="22"/>
</signal>
<signal name="LOGO_BLUE_CTRL">
<contactref element="R6-17" pad="1"/>
<contactref element="U$1" pad="20"/>
</signal>
<signal name="N$104">
<contactref element="JP0-2" pad="1"/>
<contactref element="U$1" pad="34"/>
</signal>
<signal name="LCD_SI">
<contactref element="LCD" pad="LCD_P36"/>
<contactref element="U$1" pad="15"/>
</signal>
<signal name="LCD_SCL">
<contactref element="LCD" pad="LCD_P37"/>
<contactref element="U$1" pad="17"/>
</signal>
<signal name="LCD_!RESET">
<contactref element="LCD" pad="LCD_P39"/>
<contactref element="R0-11" pad="2"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="LCD_!CS1B">
<contactref element="LCD" pad="LCD_P40"/>
<contactref element="U$1" pad="14"/>
</signal>
<signal name="N$102">
</signal>
<signal name="N$1">
<contactref element="R6-1" pad="1"/>
<contactref element="D6_1" pad="4"/>
</signal>
<signal name="N$7">
<contactref element="R6-2" pad="2"/>
<contactref element="D6_1" pad="5"/>
</signal>
<signal name="N$8">
<contactref element="R6-3" pad="2"/>
<contactref element="D6_1" pad="6"/>
</signal>
<signal name="N$3">
<contactref element="R6-7" pad="2"/>
<contactref element="D6-2" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="R6-8" pad="2"/>
<contactref element="D6-2" pad="5"/>
</signal>
<signal name="N$5">
<contactref element="R6-9" pad="2"/>
<contactref element="D6-2" pad="6"/>
</signal>
<signal name="N$22">
<contactref element="R6-4" pad="2"/>
<contactref element="D6-3" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="R6-6" pad="2"/>
<contactref element="D6-3" pad="6"/>
</signal>
<signal name="N$26">
<contactref element="R6-5" pad="2"/>
<contactref element="D6-3" pad="5"/>
</signal>
<signal name="N$27">
<contactref element="R6-12" pad="1"/>
<contactref element="D6-4" pad="6"/>
</signal>
<signal name="N$28">
<contactref element="R6-11" pad="2"/>
<contactref element="D6-4" pad="5"/>
</signal>
<signal name="N$47">
<contactref element="R6-10" pad="2"/>
<contactref element="D6-4" pad="4"/>
</signal>
<signal name="N$80">
<contactref element="R6-19" pad="1"/>
<contactref element="D6-5" pad="4"/>
</signal>
<signal name="N$81">
<contactref element="R6-20" pad="2"/>
<contactref element="D6-5" pad="5"/>
</signal>
<signal name="N$103">
<contactref element="R6-21" pad="2"/>
<contactref element="D6-5" pad="6"/>
</signal>
<signal name="N$109">
<contactref element="R6-22" pad="2"/>
<contactref element="D6-6" pad="4"/>
</signal>
<signal name="N$110">
<contactref element="R6-23" pad="2"/>
<contactref element="D6-6" pad="5"/>
</signal>
<signal name="N$111">
<contactref element="R6-24" pad="2"/>
<contactref element="D6-6" pad="6"/>
</signal>
<signal name="N$112">
<contactref element="R6-25" pad="2"/>
<contactref element="D6-7" pad="4"/>
</signal>
<signal name="N$113">
<contactref element="R6-27" pad="2"/>
<contactref element="D6-7" pad="6"/>
</signal>
<signal name="N$114">
<contactref element="R6-26" pad="2"/>
<contactref element="D6-7" pad="5"/>
</signal>
<signal name="N$115">
<contactref element="R6-30" pad="1"/>
<contactref element="D6-8" pad="6"/>
</signal>
<signal name="N$116">
<contactref element="R6-29" pad="2"/>
<contactref element="D6-8" pad="5"/>
</signal>
<signal name="N$117">
<contactref element="R6-28" pad="2"/>
<contactref element="D6-8" pad="4"/>
</signal>
<signal name="TITLE_GREEN">
<contactref element="R6-21" pad="1"/>
<contactref element="R6-24" pad="1"/>
<contactref element="R6-27" pad="1"/>
<contactref element="R6-30" pad="2"/>
<contactref element="T6-5" pad="3"/>
</signal>
<signal name="TITLE_BLUE">
<contactref element="R6-22" pad="1"/>
<contactref element="R6-19" pad="2"/>
<contactref element="R6-25" pad="1"/>
<contactref element="R6-28" pad="1"/>
<contactref element="T6-6" pad="3"/>
</signal>
<signal name="TITLE_RED">
<contactref element="R6-20" pad="1"/>
<contactref element="R6-23" pad="1"/>
<contactref element="R6-26" pad="1"/>
<contactref element="R6-29" pad="1"/>
<contactref element="T6-4" pad="3"/>
</signal>
<signal name="N$118">
<contactref element="R6-31" pad="2"/>
<contactref element="T6-4" pad="1"/>
<contactref element="R6-32" pad="2"/>
</signal>
<signal name="N$119">
<contactref element="R6-33" pad="2"/>
<contactref element="T6-5" pad="1"/>
<contactref element="R6-34" pad="2"/>
</signal>
<signal name="N$120">
<contactref element="R6-35" pad="2"/>
<contactref element="T6-6" pad="1"/>
<contactref element="R6-36" pad="2"/>
</signal>
<signal name="TITLE_RED_CTRL">
<contactref element="R6-31" pad="1"/>
<contactref element="U$1" pad="29"/>
</signal>
<signal name="TITLE_GREEN_CTRL">
<contactref element="R6-33" pad="1"/>
<contactref element="U$1" pad="28"/>
</signal>
<signal name="TITLE_BLUE_CTRL">
<contactref element="R6-35" pad="1"/>
<contactref element="U$1" pad="32"/>
</signal>
<signal name="N$121">
<contactref element="LED1-6" pad="A"/>
<contactref element="R1-19" pad="1"/>
</signal>
<signal name="N$122">
<contactref element="LED1-5" pad="A"/>
<contactref element="R1-18" pad="1"/>
</signal>
<signal name="AVCC">
<contactref element="U$1" pad="39"/>
</signal>
<signal name="USB_D-">
<contactref element="U$1" pad="26"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="USB_D+">
<contactref element="U$1" pad="27"/>
<contactref element="JP1" pad="3"/>
</signal>
<signal name="N$126">
<contactref element="LED2-5" pad="A"/>
<contactref element="R2-18" pad="1"/>
</signal>
<signal name="N$127">
<contactref element="LED2-6" pad="A"/>
<contactref element="R2-19" pad="1"/>
</signal>
<signal name="N$125">
<contactref element="R3-19" pad="1"/>
<contactref element="LED3-6" pad="A"/>
</signal>
<signal name="N$128">
<contactref element="R3-18" pad="1"/>
<contactref element="LED3-5" pad="A"/>
</signal>
<signal name="N$132">
<contactref element="LED4-5" pad="A"/>
<contactref element="R4-18" pad="1"/>
</signal>
<signal name="N$133">
<contactref element="LED4-6" pad="A"/>
<contactref element="R4-19" pad="1"/>
</signal>
<signal name="N$123">
</signal>
<signal name="N$124">
</signal>
<signal name="N$129">
</signal>
<signal name="N$130">
</signal>
<signal name="N$131">
</signal>
<signal name="N$134">
</signal>
<signal name="N$135">
</signal>
<signal name="N$136">
</signal>
<signal name="N$137">
</signal>
<signal name="N$138">
</signal>
<signal name="N$139">
</signal>
<signal name="N$140">
</signal>
<signal name="N$141">
</signal>
<signal name="N$142">
</signal>
</signals>
</board>
</drawing>
</eagle>
